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SECTION 118129

Facility Fall Protection

sales@edgefallprotection.com
www.edgefallprotection.com 


GENERAL

SECTION INCLUDES

Climbing Ladder Fall Arrest System - CLAFS


RELATED SECTIONS

Section 05500 – Metal Fabrications: Associated metal supports.

Section 05510 – Metal Stairs and Ladders.

Section 05515 – Ladders.

Section 07700 – Roof Specialties and Accessories.


REFERENCES
Occupational Safety & Health Administration (OSHA)
29 CFR 1910.23(c) (1) & 29 CFR 1926.501(b) (1) - Occupational Health and Safety Standards General Industry & Construction: Duty to have fall protection
29 CFR 1926.502(d) (15) (i-ii) - Safety and Health Regulations for Construction: Anchor Design Requirements
29 CFR 1910.66 I(c) (10), I (d) (iv), II (2) - General Industry: Anchor Design Requirements
American National Standards Institute (ANSI)
Z359.0 – Definitions and Nomenclature Used for Fall Protection and Fall Arrest.
Z359.1 – Safety Requirements for Personal Fall Arrest Systems, Subsystems and Components
Z359.2 – Minimum Requirements for a Comprehensive Managed Fall Protection Program
Z359.3 – Safety Requirements for Positioning and Travel Restraint Systems.
Z359.4 – Safety Requirements for Assisted-Rescue and Self-Rescue Systems, Subsystem and Components.
Z359.6 – Specifications and Design Requirements for Active Fall Protection Systems.
Z359.12 – Connecting Components for Personal Fall Arrest Systems
Z359.13 – Personal Energy Absorbers and Energy Absorbing Lanyards
Z359.14 – Safety Requirements for Self-Retracting Devices for Personal Fall Arrest and Rescue Systems.
Materials, Bolting, Finishing: American Society of Testing Materials (ASTM)
A36 - Standard Specification for Carbon Structural Steel.
A500 - Standard Specification for Cold-Formed Welded and Seamless Carbon Steel Structural Tubing in Rounds and Shapes
A53 - Standard Specification for Pipe, Steel, Black and Hot-Dipped, Zinc-Coated, Welded and Seamless
A325 - Standard Specification for Structural Bolts, Steel, Heat Treated, 120/105 ksi Minimum Tensile Strength
A193 - Standard Specification for Alloy-Steel and Stainless Steel Bolting for High Temperature or High Pressure Service and Other Special Purpose Applications
A123 - Standard Specification for Zinc (Hot-Dip Galvanized) Coatings on Iron and Steel Products
A666 - Standard Specification for Austenitic Stainless Steel Sheet, Strip, Plate, and Flat Bar.
American Welding Society (AWS) D1.1/D1 - Structural Welding Code – Steel
Design Standards
American Institute of Steel Construction (AISC) 325-11 [14th ed.] – Steel Construction Manual
National Design Specification (ANSI/NDS) – Wood Construction Manual
International Building Code (IBC) [2012] – Building Design Manual
American Society of Civil Engineers (ASCE/SEI) 7-10 – Minimum Design Loads for Buildings and Other Structures
American Concrete Institute (ACI) 318-11 Building Code Requirements for Structural Concrete.

SUBMITTALS

Submit under provisions of Section 01300.

Product Data:  Manufacturer's data sheets on each product to be used, including:
Preparation instructions and recommendations.
Storage and handling requirements and recommendations.
Installation methods.

Shop Drawings: Drawings showing plans, elevations, sections and details of components. Show member sizes and part identification, fasteners, anchors, fittings and evidence of compliance with structural performance requirements.
Engineering
The design shall take into consideration the potential uses of and loads on the ladder and the structure.  To be completed by the Engineer of Record.

DELIVERY, STORAGE, AND HANDLING

Deliver materials to the job site in good condition and adequately protected against damage as handrails are a finished product.

Inspect components for damage before signing the receipt from the trucking company. Truck driver must note damaged goods on the bill of lading if damaged product is found

Store products in manufacturer's unopened packaging until ready for installation.

Products to be palletized and labeled by ladder.

PROJECT CONDITIONS

Field Measurements: Where systems are indicated to fit to ladder, check actual dimensions of other construction by accurate field measurements before fabrication.

WARRANTY

Warranty: Provide manufacturer’s limited two year warranty.


PRODUCTS

MANUFACTURERS

Acceptable Manufacturer: Edge Fall Protection, LLC, which is located at in Minneapolis, MN 55419. Contact: E-mail: sales@edgefallprotection.com Website: www.edgefallprotection.com Toll Free/Fax: 844-314-1374.

Substitutions:  Not permitted.

Requests for substitutions will be considered in accordance with provisions of Section 01600.

Climbing Ladder Fall Arrest System for Roof Hatch Access


Vertical Lifeline Ladder climbing System: Provide EDGE Fall Protection LLC’s Roof Hatch Ladder Fall Arrest System. Contact: sales@edgefallprotection.com; TF/Fax: 844-314-1374. System is a Vertical lifeline System
Roof Hatch Ladder Fall Arrest System with a Telescoping Extension.
Product: Roof Hatch Ladder Fall Arrest System
System top and mid rail provided in accordance with OSHA Standards - 29 CFR 1910.23 (a)(2).
System Length: Field Verify ladder height for appropriate system length
Top and Bottom Mounting Brackets for
Steel Rung
Telescoping Pole
Pre-swagged Cable
3/8 in (9.5mm)
1x7 strand
Left, Regular Lay
Galvanized
Compliance: RR-W-410
Minimum Breaking Strength: 12,000lbs
Cable Guides: Place as needed to prevent cable abrasion
Recommended every 20-40 ft
Hollow Rung Ladder Supports
To be included on all hollow rung ladders

EXECUTION

EXAMINATION

Do not begin installation until ladders have been properly prepared and attached to substrate or structure.

If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.

PREPARATION

Clean surfaces thoroughly prior to installation.

INSTALLATION

Install in accordance with manufacturer's instructions.

PROTECTION

Protect installed products until completion of project.

Touch-up, repair or replace damaged products before Substantial Completion.
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