
PART  1   GENERAL
SECTION INCLUDES
** NOTE TO SPECIFIER ** Delete items below not required for Project.
Roof accessories of the following types:
Tubular access ladders (up to 20 feet)
Fixed access ladders (up to 30 feet)
RELATED SECTIONS
** NOTE TO SPECIFIER ** Delete any sections below not relevant to this Project; add others as required.
Section 05 50 00 - Metal Fabrications.
** NOTE TO SPECIFIER ** Roof edge protection and roof hatch protection only. Delete one or both of the following paragraphs if not required.
Section 07 41 13 - Metal Roof Panels.
Section 07 50 00 - Membrane Roofing.
REFERENCES
** NOTE TO SPECIFIER ** Delete references from the list below that are not actually required by the text of the edited Section.
California Occupational Safety & Health Administration (CAL OSHA):
CAL OSHA 1620 - Design of Temporary Railing.
CAL OSHA 1621 - Railings and Toe Boards.
CAL OSHA 1633 - Elevator Shafts to be Guarded.
CAL OSHA 3209 - Standard Guardrails.
CAL OSHA 3210 - Guardrails at Elevated Locations.
CAL OSHA 3211 - Wall Openings.
CAL OSHA 3212 - Floor Openings, Floor Holes and Roofs.
CAL OSHA 3213 - Service Pits and Yard Surface Openings.
CAL OSHA 3214 - Stair Rails and Handrails.
Occupational Safety & Health Administration (OSHA):
OSHA 29 CFR 1910.23 - Guarding Floor and Wall Openings and Holes.
OSHA 29 CFR 1910.27 - Fixed Ladders.
OSHA 29 CFR 1926.500 - Scope, Application, Definitions Applicable to this Subpart.
OSHA 29 CFR 1926.501 - Duty to Have Fall Protection.
OSHA 29 CFR 1926.502 - Fall Protection Systems Criteria and Practices.
OSHA 29 CFR 1926.503 - Training Requirements.
OSHA Warning Line Interpretations
SUBMITTALS
Submit under provisions of Section 01 30 00 - Administrative Requirements.
Product Data: Manufacturer's data sheets on each product to be used, including:
Preparation instructions and recommendations.
Storage and handling requirements and recommendations.
Installation methods.
** NOTE TO SPECIFIER ** Delete paragraph below if shop drawings not required.
Shop Drawings: Drawings showing plans, elevations, sections and details of components.
** NOTE TO SPECIFIER ** Delete selection samples if colors have already been selected.
DELIVERY, STORAGE, AND HANDLING
Deliver materials to the job site in good condition and adequately protected against damage as handrails are a finished product.
Inspect rail sections for damage before signing the receipt from the trucking company. Truck driver must note damaged goods on the bill of lading if damaged product is found.
Store products in manufacturer's unopened packaging until ready for installation.
PROJECT CONDITIONS
Field Measurements: Where handrails and railings are indicated to fit to other construction, check actual dimensions of other construction by accurate field measurements before fabrication.
WARRANTY
Warranty: Provide manufacture's two (2) year warranty.
PART  2   PRODUCTS
MANUFACTURERS
Acceptable Manufacturer: Edge Fall Protection, LLC, which is located in Minneapolis, MN. Contact: E-mail: info@edgefallprotection.com Website: www.edgefallprotection.com Toll Free/Fax: 844-314-1374.
** NOTE TO SPECIFIER ** Delete one of the following two paragraphs; coordinate with requirements of Division 1 Section on product options and substitutions.
Substitutions: Not permitted.
SYSTEMS
** NOTE TO SPECIFIER ** Delete if roof edge protection is not required.
Tubular Access Ladders: Provide fixed tubular ladder for roof elevation changes up to 20 feet. Request measurement worksheet from EDGE Fall Protection, LLC if not provided by architect.
Approved Product: EDGE Tubular Access Ladder as manufactured by EDGE Fall Protection, LLC
Standard:  Fixed ladder shall meet or exceed OSHA (Standards - 29 CFR) 1910.27
Width: as indicated on drawing
Length: as indicated on drawing
Height: as indicated on drawing
All ladders, unless otherwise indicated, required to have pass through at top of ladder for safety transitioning onto roof level. Pass through rail to be minimum 42” tall. Self-closing gate required.
Security feature as required by architect
Ladder rungs required to include non-slip element as specified by architect.
Material: 1-5/8 inch (41 mm) O.D. hot rolled pickled electric weld tubing, free of sharp edges and snag points. Mounting plates to be 2.5” x ¼” minimum
Finish: Hot-dipped galvanized
Finish: Hot-dipped galvanized with powder-coated finish
[bookmark: _GoBack]Fixed Access Ladders: Provide fixed access ladder for elevation changes up to 30 feet. Request measurement worksheet from EDGE Fall Protection, LLC if not provided by architect.
Approved Product: EDGE Fixed Access Ladder as manufactured by EDGE Fall Protection, LLC
Standard:  Fixed ladder shall meet or exceed OSHA (Standards - 29 CFR) 1910.27
Caged ladder required for heights exceeding 20 feet. When elevation change is required greater than 30 feet; landing platform required.
Width: as indicated on drawing
Length: as indicated on drawing
Height: as indicated on drawing
All ladders, unless otherwise indicated, required to have pass through at top of ladder for safety transitioning onto roof level. Pass through rail to be minimum 42” tall. Self-closing gate required.
Landing platform as specified by architect
Security feature as required by architect
Material: Side rails to be 2.5” x 3/8” galvanized steel free of sharp edges and snag points. Mounting plates to be 3” x 1/4” minimum
Provide 3/4” diameter rungs at 12” o.c. let into and fully welded for stingers
Ladder rungs required to include non-slip element as specified by architect.
Finish: Hot-dipped galvanized
Finish: Hot-dipped galvanized with powder-coated finish 
FlNlSHES
** NOTE TO SPECIFIER ** Retain one of the following two paragraphs.
Finish: Factory finished powder coat paint.
Finish: Hot dipped galvanized.
** NOTE TO SPECIFIER ** Retain one of the following two paragraphs if retaining powder coat paint.
Color: Safety yellow.
Color: Match Architect's sample.
FABRlCATlON
Assemble components with joints tightly fitted and secured. Accurately form components to suit installation.
PART  3   EXECUTION
EXAMINATION
Do not begin installation until substrates have been properly prepared.
If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
PREPARATION
Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
INSTALLATION
Install in accordance with manufacturer's instructions.
PROTECTION
Protect installed products until completion of project.
Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION
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