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SECTION 05522

Metal Guardrail and Rooftop Fall protection

sales@edgefallprotection.com
www.edgefallprotection.com 


GENERAL

SECTION INCLUDES

Non-Penetrating Enduraline Permanent Visual Warning Line System


RELATED SECTIONS

Section 05500 – Metal Fabrications: Associated metal supports.

Section 05510 – Metal Stairs and Ladders.

Section 05515 – Ladders.

Section 07700 – Roof Specialties and Accessories.

Section 07400 – Membrane Roofing: Coordination of roof edge protection installation.

Section 07411 Membrane Roof Panels: Coordination of roof edge protection installations.

REFERENCES
Occupational Safety & Health Administration (OSHA)
29 CFR 1910.23 – Guarding Floor and Wall Openings and Holes 
29 CFR 1910.27 - Fixed Ladders.
29 CFR 1926.500 - Scope, Application, and Definitions Applicable to this Subpart.
29 CFR 1926.501 - Duty to Have Fall Protection.
29 CFR 1926.502 - Fall Protection Systems Criteria and Practices.
29 CFR 1926.503 - Training Requirements.
California Occupational Safety & Health Administration (CAL OSHA)
3209 Standard Guardrails
American Welding Society (AWS) D1.1/D1 - Structural Welding Code – Steel
AWS D1.1 – Structural Welding Code – Steel.
AWS D1.3 – Structural Welding Code – Sheet Steel
Design Standards
American Institute of Steel Construction (AISC) 325-11 [14th ed.] – Steel Construction Manual
International Building Code (IBC) [2012] – Building Design Manual
American Society of Civil Engineers (ASCE/SEI) 7-10 – Minimum Design Loads for Buildings and Other Structures

SUBMITTALS

Submit under provisions of Section 01300.

Product Data:  Manufacturer's data sheets on each product to be used, including:
Preparation instructions and recommendations.
Storage and handling requirements and recommendations.
Installation methods.

Shop Drawings: Drawings showing plans, elevations, sections and details of components. Show member sizes and part identification, fasteners, anchors, fittings and evidence of compliance with structural performance requirements.

DELIVERY, STORAGE, AND HANDLING

Deliver materials to the job site in good condition and adequately protected against damage as handrails are a finished product.

Inspect rail sections for damage before signing the receipt from the trucking company. Truck driver must note damaged goods on the bill of lading if damaged product is found

Store products in manufacturer's unopened packaging until ready for installation.

Products to be palletized and labeled by roof level or designated drop zone.

PROJECT CONDITIONS

Field Measurements: Where handrails and railings are indicated to fit to other construction, check actual dimensions of other construction by accurate field measurements before fabrication.

WARRANTY

Warranty: Provide manufacturer’s limited two year warranty.

PRODUCTS

MANUFACTURERS

Acceptable Manufacturer: EDGE Fall Protection, LLC, which is located at in Minneapolis, MN 55419. Contact: E-mail: sales@edgefallprotection.com Website: www.edgefallprotection.com Toll Free/Fax: 844-314-1374.

Substitutions:  Not permitted.

Requests for substitutions will be considered in accordance with provisions of Section 01600.

Rooftop Fall Protection


Non-Penetrating Enduraline Permanent Visual Warning Line System: Provide EDGE Fall Protection LLC’s Enduraline Visual Warning Line System. Contact: Sales@edgefallprotection.com; TF/Fax: 844-314-1374. System is a non-penetrating freestanding pedestrian visual warning line barrier system on roof, including railing sections, weighted base plates and accessories in the configuration and locations indicated on the Drawings.
Product: Enduraline Visual Warning Line System by EDGE Fall Protection.
Warning Line: Galvanized aircraft cable with polyurethane coating
Sag no less than 34”, and no higher than 39”
Powder coated yellow visual warning line spaced every 6’ OC
Mounting Bases: 104# Class 30 gray iron material cast.  Rubber pads are standard on bottom of bases.
Receiving posts: option of (2) or (4) receiving posts.
Receiver Posts: Provided with a positive pin locking system into base and rail interface that allow rails to be mounted in any direction. Receiver posts shall have drain holes.
Rail Accessories: 
Standard connection to EDGE 360 Mobile Safety Rail
Securing Pins: 1010 carbon steel, zinc plated and yellow chromate dipped. Pins shall consist of collared pin and latch that connects to lynch pin.
Roof Accessories:
Roof Pads: Provide EPDM Roof Pad under each base to protect roof membrane.
Base Mover: Provide Base Mover, Part #400062 two-wheeled steel cart to transport one base unit.

EXECUTION

EXAMINATION

Do not begin installation until ladders have been properly prepared and attached to substrate or structure.

If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.

PREPARATION

Clean surfaces thoroughly prior to installation.

INSTALLATION

Install in accordance with manufacturer's instructions.

PROTECTION

Protect installed products until completion of project.

Touch-up, repair or replace damaged products before Substantial Completion.


END OF SECTION
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