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SECTION 05522

Metal Guardrail and Rooftop Fall protection

sales@edgefallprotection.com
www.edgefallprotection.com 


GENERAL

SECTION INCLUDES

Non-Penetrating EDGE 360 Mobile Hide-A-Rail Passive Fall Restraint


RELATED SECTIONS

Section 05500 – Metal Fabrications: Associated metal supports.

Section 05510 – Metal Stairs and Ladders.

Section 05515 – Ladders.

Section 07700 – Roof Specialties and Accessories.

Section 07400 – Membrane Roofing: Coordination of roof edge protection installation.

Section 07411 Membrane Roof Panels: Coordination of roof edge protection installations.

REFERENCES
Occupational Safety & Health Administration (OSHA)
29 CFR 1910.23 – Guarding Floor and Wall Openings and Holes 
29 CFR 1910.27 - Fixed Ladders.
29 CFR 1926.500 - Scope, Application, and Definitions Applicable to this Subpart.
29 CFR 1926.501 - Duty to Have Fall Protection.
29 CFR 1926.502 - Fall Protection Systems Criteria and Practices.
29 CFR 1926.503 - Training Requirements.
California Occupational Safety & Health Administration (CAL OSHA)
3209 Standard Guardrails
American Welding Society (AWS) D1.1/D1 - Structural Welding Code – Steel
AWS D1.1 – Structural Welding Code – Steel.
AWS D1.3 – Structural Welding Code – Sheet Steel
Design Standards
American Institute of Steel Construction (AISC) 325-11 [14th ed.] – Steel Construction Manual
International Building Code (IBC) [2012] – Building Design Manual
American Society of Civil Engineers (ASCE/SEI) 7-10 – Minimum Design Loads for Buildings and Other Structures

SUBMITTALS

Submit under provisions of Section 01300.

Product Data:  Manufacturer's data sheets on each product to be used, including:
Preparation instructions and recommendations.
Storage and handling requirements and recommendations.
Installation methods.

Shop Drawings: Drawings showing plans, elevations, sections and details of components. Show member sizes and part identification, fasteners, anchors, fittings and evidence of compliance with structural performance requirements.

DELIVERY, STORAGE, AND HANDLING

Deliver materials to the job site in good condition and adequately protected against damage as handrails are a finished product.

Inspect rail sections for damage before signing the receipt from the trucking company. Truck driver must note damaged goods on the bill of lading if damaged product is found

Store products in manufacturer's unopened packaging until ready for installation.

Products to be palletized and labeled by roof level or designated drop zone.

PROJECT CONDITIONS

Field Measurements: Where handrails and railings are indicated to fit to other construction, check actual dimensions of other construction by accurate field measurements before fabrication.

WARRANTY

Warranty: Provide manufacturer’s limited two year warranty.


PRODUCTS

MANUFACTURERS

Acceptable Manufacturer: EDGE Fall Protection, LLC, which is located at in Minneapolis, MN 55419. Contact: E-mail: sales@edgefallprotection.com Website: www.edgefallprotection.com Toll Free/Fax: 844-314-1374.

Substitutions:  Not permitted.

Requests for substitutions will be considered in accordance with provisions of Section 01600.

Roof Hatch Safety Rail Guardrail


Roof Hatch Safety Rail: Provide EDGE Roof Hatch Guardrail freestanding pedestrian egress barrier system around roof hatch by EDGE Fall Protection, LLC. Contact: Sales@edgefallprotection.com ; TF/Fax: 844-314-1374.
EDGE Roof Hatch Guardrail – Non-Penetrating
System shall have top and mid rail in accordance with OSHA Standards - 29 CFR 1910.23 (a)(2).
Structural Load: 200 lb (90.7 kg), minimum, in any direction to all components in accordance with OSHA Regulation 29 CFR 1926.502.
Height: 42 inches (1067 mm), nominal.
EDGE HatchGuard Frame: 2” x 2” 14 gauge steel with 1-5/8” mid rails
Connections: (4) HHCS ½”-13 Hex bolts with foot pads to clamp onto the curb of the roof hatch
Grab Bars welded onto frame of Roof Hatch Guardrail
24” clearance provided for entry and exit of roof hatch
Self-closing safety gate provided; capable of being mounted in either direction.
Sizing:
Roof Hatch Size (W x L): 30 x 54 in (762 x 1372 mm).
Roof Hatch Size (W x L): 30 x 96 in (762 x 2438 mm).
Roof Hatch Size (W x L): 36 x 30 in (914 x 762 mm).
Roof Hatch Size (W x L): 36 x 36 in (914 x 914 mm).
Roof Hatch Size (W x L): 48 x 48 in (1219 x 1219 mm).
Roof Hatch Size (W x L), (in / mm): ______.
As Specified by Architect
Assembly Options
Architect to specify assembly option
Fully Welded
Field bolt-on assembly
No drilling into hatch or roof. Elastomeric tipped compression bolts are tightened against the curb of the roof hatch.
Finish: Steel Surfaces
Hot Dip Zinc Galvanized
Factory finished powder coat paint
Hot Dip Zinc Galvanized & Factory Finished powder coat paint
Color:
None
Safety Yellow
Color Specified by Architect

EXECUTION

EXAMINATION

Do not begin installation until ladders have been properly prepared and attached to substrate or structure.

If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.

PREPARATION

Clean surfaces thoroughly prior to installation.

INSTALLATION

Install in accordance with manufacturer's instructions.

PROTECTION

Protect installed products until completion of project.

Touch-up, repair or replace damaged products before Substantial Completion.


END OF SECTION
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